Large battery enclosures made from plastic series-ready

•	Feasibility of plastic enclosures for high-voltage batteries in electric vehicles proven
•	Technology demonstrator passes all important mechanical and thermal tests
•	Prototype testing in an electric test vehicle
•	Launch of development projects for series production with automotive manufacturers

Cologne, October 12, 2022 – Technical plastics such as polyamide 6 offer numerous benefits for the design of battery enclosures for electric vehicles – in terms of sustainability, manufacturing costs, weight savings and economical functional integration, for example. However, there were previously lingering doubts as to whether these large and complex components are also able to meet the very demanding requirements in relation to mechanical strength and flame-retardant properties. Kautex Textron and LANXESS have now carried out a comprehensive examination of precisely this using a jointly developed technology demonstrator made from polyamide 6. LANXESS was responsible for the material development and Kautex Textron for the engineering, design and the manufacturing process of the demonstrator. 

“The near-series demonstrator passes all mechanical and thermal tests that are relevant for such enclosures. In addition, solutions for the thermal management and leak tightness of the enclosure, for example, have been developed. This all has proven the technical feasibility of these safety components, which are complex and subject to high levels of stress,” explains Dr. Christopher Hoefs, Project Manager e-Powertrain at LANXESS. At the moment, an enclosure prototype is being road tested in a test vehicle to verify its suitability for daily use. “We are currently jointly tackling the first series-production development projects with automotive manufacturers in order to implement the new technology in series production,” explains Felix Haas, Director Product Development at Kautex Textron. 

Smaller carbon footprint

“Calculations revealed that the carbon footprint of the plastic enclosure is over 40 percent smaller compared to an aluminum design. The lower energy use in the production of polyamide 6 compared with metal as well as other factors – such as the omission of time-consuming cathodic dip painting to prevent corrosion where steel is used – help to minimize the carbon footprint,” says Hoefs. The thermoplastic component design also makes recycling the enclosure easier compared with thermoset materials such as sheet molding compounds (SMC), for example.

Highly durable, resistant to external fire sources

The tests on the technology demonstrator were carried out in accordance with internationally recognized standards for battery-powered electric vehicles such as ECE R100 from the Economic Commission for Europe or the Chinese standard GB 38031. The large-format all-plastic enclosure, which measures around 1,400 millimeters in both length and width, demonstrated its performance in all relevant tests. For example, it meets the requirements of the mechanical shock test, which is used to examine the component’s behavior in the event of severe shocks, and of the crush test, which the developers use to examine the resistance of the battery enclosure in the event of slow deformation. The results of the drop and vibration tests were also positive, as were those of the bottom impact test. This test examines the stability of the batteries, which are mostly accommodated in the vehicle floor, in the event of a ground contact of the vehicle structure or of impacts from sizeable stones. “All test results corroborate the previous simulations and calculations. A critical failure of the plastic enclosure would not have occurred in any of the load cases,” explains Haas. The demonstrator also proved its resistance to external sources of fire underneath the vehicle in accordance with ECE R100 (external fire).

Lower weight, lower manufacturing costs 

The demonstrator was developed based on the aluminum battery housing of a mid-size electric vehicle and designed for mass production. It is manufactured in a single-stage compression molding process with a molding compound based on the polyamide 6 compound Durethan B24CMH2.0 from LANXESS and does not require any further rework. Crash-relevant areas are specially reinforced with locally placed blanks made from the continuous-fiber-reinforced, polyamide 6-based composite Tepex dynalite 102-RGUD600. Compared with an aluminum design, there is a weight saving of around 10 percent, which is advantageous for the range and therefore the carbon footprint of the vehicle. The integration of functions – such as the fasteners, reinforcing ribs and components for the thermal management – reduces the number of individual components significantly compared with the metal design, which simplifies assembly and logistical effort and reduces manufacturing costs. 

You can find more detailed information about LANXESS products and technologies for the field of new mobility and battery innovations from Kautex Textron at https://lanxess.com/en/Products-and-Solutions/Focus-Topics/LANXESS-e-Mobility and www.kautex.com/en/mobility/battery-systems. 

LANXESS is a leading specialty chemicals company with sales of EUR 6.1 billion in 2021. The company currently has about 13,200 employees in 33 countries. The core business of LANXESS is the development, manufacturing and marketing of chemical intermediates, additives and consumer protection products. LANXESS is listed in the leading sustainability indices Dow Jones Sustainability Index (DJSI World and Europe) and FTSE4Good.

Forward-Looking Statements
This company release contains certain forward-looking statements, including assumptions, opinions, expectations and views of the company or cited from third party sources. Various known and unknown risks, uncertainties and other factors could cause the actual results, financial position, development or performance of LANXESS AG to differ materially from the estimations expressed or implied herein. LANXESS AG does not guarantee that the assumptions underlying such forward-looking statements are free from errors, nor does it accept any responsibility for the future accuracy of the opinions expressed in this presentation or the actual occurrence of the forecast developments. No representation or warranty (expressed or implied) is made as to, and no reliance should be placed on, any information, estimates, targets and opinions contained herein, and no liability whatsoever is accepted as to any errors, omissions or misstatements contained herein, and accordingly, no representative of LANXESS AG or any of its affiliated companies or any of such person's officers, directors or employees accepts any liability whatsoever arising directly or indirectly from the use of this document.

Information for editors:
All LANXESS news releases and their accompanying photos can be found at http://press.lanxess.com. Recent photos of the Board of Management and other LANXESS image material are available at http://photos.lanxess.com. 

You can find further information concerning LANXESS chemistry at http://lanxess.com/en/Media/Stories

Follow us on Twitter, Facebook, LinkedIn and YouTube:

http://www.twitter.com/LANXESS
http://www.facebook.com/LANXESS
http://www.linkedin.com/company/lanxess
http://www.youtube.com/lanxess